CALLISTO status report #12, Revision A of 2004-12-14

To:
Arnold O. Benz	ETHZ	benz@astro.phys.ethz.ch	
Tim Bastian	NRAO	tbastian@nrao.edu	
Richard F. Bradley	NRAO	rbradley@nrao.edu	
Erin Mastrantonio	NRAO	emastran@nrao.edu	
Peter Messmer	TXCORP	messmer@txcorp.com	
Hansueli Meyer	ETHZ	meyerh@astro.phys.ethz.ch	
Hanspeter Hächler	ETHZ	haechler@phys.ethz.ch	

From:
Christian Monstein	ETHZ	monstein@astro.phys.ethz.ch	

Host-PC
Although a lot of tests were made with the last version of 2004-12-07 new errors were accidentally included (sorry for that). These errors have been solved and are now implemented in a new software version V1.21. The complete set of files is available as ZIP file under http://www.astro.phys.ethz.ch/instrument/callisto/Appdocs/20041214.ZIP
In note form all changes that have been implemented in present Callisto-software:
•	No software crash if a pre-chosen frequency file is no more available
•	Set focus code correctly, even the FPU is missing.
•	Frequency x-axis label restricted to “%5.1f”
•	Complete disabled communication to a ‘non-existing’ FPU. (Serial communication to/with a non-existing FPU leads to strange behavior of the whole system…).
•	New function implemented ‘Overview commands’ to save all 13200 channels in the logfile which afterwards may be analyzed by EXCEL, IDL, Math-CAD or whatever tool that can read ASCII files and produce XY-plots.

List of files which must be in the callisto working-directory:
-	callisto.exe
-	callisto.cfg
-	scheduler.cfg
-	frq00201.cfg
-	CFITSIO.DLL
-	CW3230.DLL
-	WSC32.DLL
-	CallistoHints.pdf
-	CallistoOPmanual.pdf
-	All other files are used for software engineering only, they may be deleted